NV3/NV3T/NV4 hardware cursor

Unlock extended CRTC registers

CIO_CRE_HCUR_ADDR0
	Bits [6:0] 	= Address

CIO_CRE_HCUR_ADDR1
	Bits [7:3]	= Bits [11:7] of address
	Bit 1		= Cursor Doubling
	Bit 0		= Enable

PRAMDAC_CU_START_POS (MMIO 0x680300)
	Bits [11:0]	= X Pos
	Bits [27:16]	= Y Pos

CursorAddress >> 16 written to addr0
(((CursorAddress >> 11) & 0x1F) << 3) | 1 (for enable) written to addr1

Lock extended CRTC registers
Enable - write 